1. Rename **Top** layer to **Breadboard** colour **Cyan**.
2. Paste breadboard outline from “breadboard.dip” and lock it.
3. Go to **Design Rules** and check Real time DRC and **Check jumper Wires** under **Option tab**.
4. Start placing components.
5. Routing:
6. *Breadboard* to be routed over only on *breadboard outlines*.
7. *Bottom* NOT to be routed over *breadboard outlines*.
8. *Bottom* Trace length only equal to 0.1in, i.e. only adjacent Breadboard lines can be joined.
9. Error check:
10. Hover mouse over a pad, all other pads on that bb line should highlight to red.